org.eclipse.jetty.websocket

## Interface WebSocket.FrameConnection

- All Superinterfaces:
    WebSocket.Connection
  All Known Implementing Classes:
    WebSocketConnectionD00, WebSocketServletConnectionD00
  Enclosing interface:
    WebSocket

      public static interface WebSocket.FrameConnection
      extends WebSocket.Connection

  Frame Level Connection

  The Connection interface at the level of sending/receiving frames rather than messages. Also contains methods to decode/generate flags and opcodes without using constants, so that code can be written to work with multiple drafts of the protocol.

- - ### Method Summary

    Methods
    Modifier and Type | Method and Description
    --- | ---
    `byte` | `binaryOpcode()`
    `byte` | `continuationOpcode()`
    `byte` | `finMask()`
    `boolean` | `isAllowFrameFragmentation()`
    `boolean` | `isBinary(byte opcode)`
    `boolean` | `isClose(byte opcode)`
    `boolean` | `isContinuation(byte opcode)`
    `boolean` | `isControl(byte opcode)`
    `boolean` | `isMessageComplete(byte flags)`
    `boolean` | `isPing(byte opcode)`
    `boolean` | `isPong(byte opcode)`
    `boolean` | `isText(byte opcode)`
    `void` | `sendControl(byte control, byte[] data, int offset, int length)` Send a control frame
    `void` | `sendFrame(byte flags, byte opcode, byte[] data, int offset, int length)` Send an arbitrary frame
    `void` | `setAllowFrameFragmentation(boolean allowFragmentation)` Set if frames larger than the frame buffer are handled with local fragmentations
    `byte` | `textOpcode()`

    - ### Methods inherited from interface org.eclipse.jetty.websocket.WebSocket.Connection

      `close, close, disconnect, getMaxBinaryMessageSize, getMaxIdleTime, getMaxTextMessageSize, getProtocol, isOpen, sendMessage, sendMessage, setMaxBinaryMessageSize, setMaxIdleTime, setMaxTextMessageSize`

- - ### Method Detail

    - #### binaryOpcode

          byte binaryOpcode()

      Returns:
        The opcode of a binary message

    - #### textOpcode

          byte textOpcode()

      Returns:
        The opcode of a text message

    - #### continuationOpcode

          byte continuationOpcode()

      Returns:
        The opcode of a continuation frame

    - #### finMask

          byte finMask()

      Returns:
        Mask for the FIN bit.

    - #### setAllowFrameFragmentation

          void setAllowFrameFragmentation(boolean allowFragmentation)

      Set if frames larger than the frame buffer are handled with local fragmentations
      Parameters:
        `allowFragmentation` -

    - #### isMessageComplete

          boolean isMessageComplete(byte flags)

      Parameters:
        `flags` - The flags bytes of a frame
      Returns:
        True of the flags indicate a final frame.

    - #### isControl

          boolean isControl(byte opcode)

      Parameters:
        `opcode` -
      Returns:
        True if the opcode is for a control frame

    - #### isText

          boolean isText(byte opcode)

      Parameters:
        `opcode` -
      Returns:
        True if the opcode is for a text frame

    - #### isBinary

          boolean isBinary(byte opcode)

      Parameters:
        `opcode` -
      Returns:
        True if the opcode is for a binary frame

    - #### isContinuation

          boolean isContinuation(byte opcode)

      Parameters:
        `opcode` -
      Returns:
        True if the opcode is for a continuation frame

    - #### isClose

          boolean isClose(byte opcode)

      Parameters:
        `opcode` -
      Returns:
        True if the opcode is a close control

    - #### isPing

          boolean isPing(byte opcode)

      Parameters:
        `opcode` -
      Returns:
        True if the opcode is a ping control

    - #### isPong

          boolean isPong(byte opcode)

      Parameters:
        `opcode` -
      Returns:
        True if the opcode is a pong control

    - #### isAllowFrameFragmentation

          boolean isAllowFrameFragmentation()

      Returns:
        True if frames larger than the frame buffer are fragmented.

    - #### sendControl

          void sendControl(byte control,
                         byte[] data,
                         int offset,
                         int length)
                           throws IOException

      Send a control frame
      Parameters:
        `control` -
        `data` -
        `offset` -
        `length` -
      Throws:
        `IOException`

    - #### sendFrame

          void sendFrame(byte flags,
                       byte opcode,
                       byte[] data,
                       int offset,
                       int length)
                         throws IOException

      Send an arbitrary frame
      Parameters:
        `flags` -
        `opcode` -
        `data` -
        `offset` -
        `length` -
      Throws:
        `IOException`

Copyright © 1995-2015 Mort Bay Consulting. All Rights Reserved.